**Condition of all closing appliances**

**For vessels returning to active duty after getting laid-up**

**5 years for protected @ cladded shafts and corrosion resistant materials**

**Boilers > 3.4 bar**

**Interval of 2.5 years**

**5 years for oil lubricated bearings**

**3-4 years for unprotected carbon steel shafts**

**All requirements of special periodical surveys**

**Cycle of 5 years**

**Lloyds register only**

**5 years intervals**

**Details of compartments**

**Hull thickness and material**

**May alternately replace docking surveys**

**Applicable to ships with high resistance paint only**

**rudder**

**Stern frame**

**External & through hull fittings**

**Intervals of 2.5 years**

**Shell plating**

**5 years for freshwater operators**

**Operating systems in tankers, chemical and LNG carriers**

**Main and auxiliary machines**

**Cargo holds in vessels >15 years**

**6 months after annual surveys**

**1 year intervals**

**Cargo holds**

**Anchors and cables**

**Structural fire protection**

**Watertight doors and bulkheads**

REACTIVATION SURVEYS

BOILER SURVEYS

TAILSHAFT SURVEYS

CONTINUOUS SURVEYS

SPECIAL SURVEYS

IN-WATER SURVEYS

DOCKING SURVEYS

INTERMEDIATE SURVEYS

ANNUAL SURVEYS

**PERIODICAL SURVEYS**